Central Office Code Assignment Guidelines (COCAG)

Central Office Code (NXX) Assignment Request - Part 2, Form 1

**Revised: June 12, 2015**

Following are CO Code (NXX) data requirements for the iconectiv BIRRDS database. Section 1.2 of the COCAG/TBPAG Forms Part 2 Job Aid may be referenced for assistance in completing this form. This form must always be completed for newly assigned CO Codes.

**New CO Code** All items are required unless otherwise noted.

**Data change** Items 1-5 are required, as are the appropriate element(s) to be changed.

**Disconnect**  Only items 1-5 should be provided.

1. **NPA** Click here to enter text.

Number Plan Area Code (Area Code) in which the CO Code (NXX)has been assigned.

1. **NXX** Click here to enter text.

Central Office Code (the assigned NXX).

1. **BLOCK ID** A

No entry required for CO Codes (always “A”).

1. **STATUS** Click here to enter text.

E = new code, M = change to supporting data, D = disconnect.

1. **EFF DATE** Click here to enter text.

Date that a new CO code can first be routed to, date that supporting data change will be effective, or date of disconnect.

1. **OCN** Click here to enter text.

Operating Company Number.

1. **LOCALITY** Click here to enter text. Locality in **RATE CENTER** Click here to enter text.

(max 10 characters each).

1. **INDX** Click here to enter text.

An index to distinguish cases of multiple same-name LOCALITY in the STATE/PROVINCE, if applicable.

1. **STATE/PROV** Click here to enter text.

Two-character code for the state, territory, or province of the LOCALITY.

1. **PLNAME (10)** Click here to enter text.

PLACENAME in same RATE CENTER as LOCALITY (max 10 characters[[1]](#footnote-1)).

1. **COTYPE** Click here to enter text.

Identifies use of the CO Codes [Chose one – EOC, PLN, PMC, RCC, SIC, TST, SP1, SP2, VOI, (for ODDBALL CODES see Job Aid)].

1. **SSC** Click here to enter text.

Special Service Code – [Choose one (or valid combinations up to 4) – A,B,C,I,J,M,N,O,R,S,T,V,W,X,Z,8].

1. **TR DIG EO** Click here to enter text.

Number of digits to be outpulsed to a switching entity/POI end office by another carrier (e.g., NPA + NXX + line would be 10).

1. **TR DIG AT** Click here to enter text.

Number of digits to be outpulsed to a switching entity/POI tandem office by another carrier (e.g., NPA + NXX + line would be 10).

1. **NXXTYPE** Click here to enter text.

Identifies use of CO Code (NXX). (Choose one of listed values provided in the COCAG Part 2 Job Aid).

1. **BILL RAO** Click here to enter text.

Enter a valid Revenue Accounting Office code.

1. **BO Code** Click here to enter text.

Enter an appropriate Business Office code.

1. **CO Type** Click here to enter text.

Company Type – (Choose appropriate value 0-9 provided in the COCAG Part 2 Job Aid).

1. **TIME ZONE** Click here to enter text.

0-none, 1-Guam/CNMI, 2-Hawaii/American Samoa, 3-Alaska, 4-Pacific, 5-Moutain, 6-Central, 7-Eastern, 8-Atlanic, 9-Newfoundland.

1. **IDDD** Click here to enter text.

International Direct Distance Dialing. [Y- if the CO Code (NXX) can place IDDD calls, N – if not].

1. **DIND** Click here to enter text.

Dialable Indicator. (Y if directly dialable, N if not).

1. **DAYLIGHT** Click here to enter text.

[Y – if the CO Code (NXX) serves an area that observes daylight saving, N – if not].

1. **PORTABLE** Click here to enter text.

(Y/N) Y if line number can be ported from this CO Code.

1. **TEST LINE Information:**

**TEST LINE** Click here to enter text.

Four-digit test line number (i.e., NPA-NXX-xxxx).

**RESPONSE** Click here to enter text.

Response from TEST LINE (A=Announcement, M=Miliwatt).

**EXP DATE** Click here to enter a date.

Optional, butif used must be at least 175 days after the CO Code establish (STATUS “E”) EFF Date.

1. **IP CAPABLE** Click here to enter text.

(Y/N) Y if the Code Holder has chosen to identify that any non-ported lines within the NPA-NXX can be routed via IP.

1. **SWITCH** Click here to enter text.

Eleven character CLLITM[[2]](#footnote-2) code that identifies the switching entity/POI (see COCAG Part 2, Form 2 if switch has not yet been established in BIRRDS).

1. **SHA IND** Click here to enter text.

Switch Homing Arrangement (two digits) (multiple homing arrangements – see COCAG Part 2, Form 8 if SHA IND has not yet been established in BIRRDS for the given switch) (if not applicable, enter 00).

1. If greater than 10 characters, an abbreviated (10 character) PLACENAME will be created and reported to meet requirements of some billing systems. [↑](#footnote-ref-1)
2. CLLI is a trademark of Telcordia Technologies, Inc. dba iconectiv. [↑](#footnote-ref-2)