Central Office Code Assignment Guidelines (COCAG)

Central Office Code (NXX) Assignment Request - Part 2, Form 2

**Revised: September 5, 2014**

Switching Entity/POI (Point of Interconnection) data requirements for the iconectiv BIRRDS database. Section 1.3 of the COCAG/TBPAG Forms Part 2 Job Aid may be referenced for assistance in completing this form.

**New Switching Entity/POI** All items are required unless otherwise noted.

**Data change** Items 1-3 are required, as are the appropriate element(s) to be changed.

**Disconnect**  Only items 1-3 should be provided.

1. **SWITCH** Click here to enter text.

A switch code - 11 characters (e.g. CLLI[[1]](#footnote-1)™). For Central Office Code assignments, this is the switching entity/POI that will originate and terminate calls from/to the assigned CO Code.

1. **STATUS**Click here to enter text.

E = new entity/POI, M = change to supporting data, D = disconnect.

1. **EFF Date** Click here to enter a date.

Date a new switching entity/POI can be routed to, date supporting data change will be effective or, date of disconnect (mm/dd/yy).

1. **EQPT TYPE** Click here to enter text.

A valid code designating the specific equipment being used.

1. **OCN** Click here to enter text.

Operating Company Number.

1. **LATA** Click here to enter text.

Local Access Transport Area Code (3 digits, 5 may apply in Florida).

1. **VC** Click here to enter text.

The appropriate Vertical Coordinate for the switching entiry/POI.

1. **HC** Click here to enter text.

The appropriate Horizontal Coordinate for the switching entity/POI.

1. **IDDD** Click here to enter text.

International Direct Distance Dialing (Y - if the switching entity/POI permits IDDD, N - if not).

1. **Address Data** (should identify the actual location of the switching entity/POI)

**Street** Click here to enter text.

**City** Click here to enter text. **State/Prov**Click here to enter text.

**Postal Code** Click here to enter text.

1. **Inter LATA use** (default N) (Y/N) Click here to enter text.
2. **Point Code** (Optional) Click here to enter text.
3. **Class 4/5 Office** Click here to enter text.

(CLLI of the “other” side of such offices, if applicable).

1. **Intercompany EOC Use** (default N) (Y/N) Click here to enter text.
2. **Homing Arrangements**

As may be applicable, enter the appropriate eleven character SWITCH (e.g., CLLI) to which the switching entity/POI may home to for various feature group capabilities, signaling, etc.

|  |  |  |
| --- | --- | --- |
| **ORIGINATING** | **TERMINATING** | **ADDITIONAL** |
| **FG B TDM**  Click here to enter text. | **FG B TDM**  Click here to enter text. | **HOST**  Click here to enter text. |
| **FG C TDM**  Click here to enter text. | **FG C TDM**  Click here to enter text. | **STP 1**  Click here to enter text. |
| **FG D TDM**  Click here to enter text. | **FG D TDM**  Click here to enter text. | **STP 2**  Click here to enter text. |
| **OS TDM**  Click here to enter text. | **OS TDM**  Click here to enter text. |  |
| **FGB INT**  Click here to enter text. | **FGB INT**  Click here to enter text. | **800 SSP**  Click here to enter text. |
| **FG C INT**  Click here to enter text. | **FG C INT**  Click here to enter text. | **ISDN FS OFC**  Click here to enter text. |
| **FG D INT**  Click here to enter text. | **FG D INT**  Click here to enter text. | **ACTUAL SW ID**  Click here to enter text. |
| **LOCAL TDM**  Click here to enter text. | **LOCAL TDM**  Click here to enter text. | **CALL AGENT**  Click here to enter text. |
| **INTA TDM**  Click here to enter text. | **INTRA TDM**  Click here to enter text. | **TRUNK GATEWAY**  Click here to enter text. |
| **CS DATA TDM**  Click here to enter text. | **CS DATA TDM**  Click here to enter text. |  |

1. **Switching Entity/POI**

Enter an "X" next to all functionalities that apply. (At least one functionality must be flagged.)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **END OFC** | **FG B TDM** | **BCR5** | **STP** | **SW56** |
| **HOST** | **FG C TDM** | **BCR6** | **CCS AC OFC** | **FGD 56** |
| **REMOTE** | **FG D TDM** | **PRI 64** |  | **FGD 64** |
| **DA OFC** | **OS TDM** | **ISDN MULTIRT** | **800 SSP** | **INTRA PRSUB** |
| **CLASS 4/5** | **INTERMED OFC** | **ISDN FS OFC** | **LNP CAPABLE** | **CALL AGENT** |
| **WIRELESS OFC** | **DA TDM** |  |  | **TRNK GATEWAY** |
|  | **911 TANDEM** |  |  | **ACSS GATEWAY** |
|  |  |  |  |  |
|  | **LOCAL TDM** |  | **CIP** |  |
|  | **INTRA TDM** |  | **CSP** |  |
|  | **CS DATA TDM** |  |  |  |

1. **RAO** Click here to enter text.

An appropriate Revenue Accounting Office Code if the switch is a FG B, FG C, FG D, or OS TDM (tandem).

1. ™ CLLI is a trademark of Telcordia Technologies, Inc. dba iconectiv. [↑](#footnote-ref-1)