Central Office Code Assignment Guidelines (COCAG)

Central Office Code (NXX) Assignment Request - Part 2, Form 7

**Revised: June 12, 2015**

Following are Location Routing Number (LRN) data requirements for the iconectiv BIRRDS database. Section 1.5.1 of the COCAG Forms Part 2 Job Aid may be referenced for assistance in completing this form.

 **New LRN** All items are required unless otherwise noted.

 **Data change** Items 1-3 are required, as are the appropriate element(s) to be changed.

 **Disconnect** Only items 1-3 should be provided.

1. **LRN** Click here to enter text.

Ten digit Location Routing Number (LRN) associated with a given switching entity/POI.

1. **STATUS** Click here to enter text.

E = newly established LRN, M = change to supporting data D = disconnect of an LRN.

1. **EFF DATE** Click here to enter a date.

Date the LRN can first be routed to, date supporting data change will be effective or, date of disconnect (mm/dd/yy).

1. **IP CAPABLE OCN** Click here to enter text.

Optional. The Code Holder has chosen to identify the OCN of a company to which IP traffic can be routed.

1. **LATA Served** Click here to enter text.

Local Access Transport Area code (3 digits, 5 may apply in Florida) to which the LRN is associated.

1. **RATE CENTER** Click here to enter text.

Optional. Identifies the exchange Rate Center served by the CO Code (NXX) (maximum of 10 characters).

1. **RC TYPE** Click here to enter text.

Optional. If applicable, enter an indicator for the type of Rate Center (choose one S=Suburban, Z=Zoned).

1. **RC STATE/PROV** Click here to enter text.

Optional. Two character code for the state, territory, or province of the Rate Center.